**20” RUBBISH CHUTE – BRACKETS & CHAIN**

* Chain is 7mm x 42mm grade 30 long link chain
* Chain manufactured to BS 6405
* Minimum breaking load as 1.9t, maximum service load in this application is 480kg
* Bracket is made from mild steel
* Tests indicate that there is no distortion of the bracket at maximum load of 480kg, the bracket fails at around 1.1t